# Some basic logging
LogLevel 3
LogDestination x-syslog:///LOG_DAEMON
# Prevents RADIUS servers from causing a loop by sending requests back again.
LoopPrevention On
# FTICKS is a standardised way of logging authentication attempts.
FTicksSyslogFacility LOG_LOCAL0
FTicksReporting Full
FTicksMAC VendorKeyHashed
FTicksKey arandomsalt
# Upstream RADIUS proxies
server roaming0.govroam.uk {
host 212.219.190.139
type udp
secret XXXX
statusServer on #This checks that status of the adjacent servers.
}
server roaming1.govroam.uk {
host 212.219.209.43
type udp
secret XXXX
statusServer on
}
server roaming2.govroam.uk {
host 212.219.247.59
type udp
secret XXXX
statusServer on
}
server roaming3.govroam.uk {
host 195.194.21.203
type udp
secret XXXX
statusServer on
}
# IdP for local realm
server idp.localnet.nhs.uk {
host 1.1.1.1
type udp
secret XXXX
}
# RADIUS requests will also be received from the national proxies. (Omit for Visited Only)
client roaming0.govroam.uk {
host 212.219.190.139
type udp
secret XXXX
}
client roaming1.govroam.uk {
host 212.219.209.43
type udp
secret XXXX
}
client roaming2.govroam.uk {
host 212.219.247.59
type udp
secret XXXX
}
client roaming3.govroam.uk {
host 195.194.21.203
type udp
secret XXXX
}
# Wireless system
client nas {
host 10.10.10.10
type udp
secret XXXX
fticksVISCOUNTRY GB
fticksVISINST 1localnet.nhs.uk # Adding information to the logs about this client.
}
#Known local realm (Omit for Visited Only)
realm localnet.nhs.uk {
server idp.localnet.nhs.uk
AccountingResponse On
}
#Default destination for unknown realms
realm * {
server roaming0.govroam.uk
server roaming1.govroam.uk
server roaming2.govroam.uk
server roaming3.govroam.uk
AccountingResponse On
}