Configuring F-TICKS for FreeRADIUS is as simple as adding an extra module file and restarting FR. This is an F-TICKS code fragment which should work and be of the right format.

The F-TICKS logs will be sent to syslog and processed according to your syslog configuration.

To send the F-TICKS to Jisc your syslog configuration will need to be able to identify the right messages and know where to send them.

Destination: utilities.govroam.uk, port 514.

An easy way to identify the messages would be to look for 'F-TICKS' in the message.

Example for syslog-ng:

destination d_jisc {
syslog("utilities.govroam.uk" transport("tcp") port("514"));
};
filter f_fticks {
facility(local0) and match ("F-TICKS", value ("MESSAGE"));
};
log {
source(s_src);
filter(f_fticks);
destination(d_jisc);
};