Adding Operator-Name

Cisco ISE doesn't insert O-N into the Request by default. O-N helps Home sites identify where their users' authentications are coming from. Combined with Chargeable User Identity, Home and Visited sites can provide and follow an audit trail back to a user without the Visited site knowing the users' details.

Adding the Operator-Name attribute

Go to Policy → Policy Elements → Dictionaries.

Open up the System dropdown.

Open up the Radius dropdown.

Click on IETF.

Click on unknown-126 and enter

Attribute Name as 'Operator-Name'

Data Type as STRING

Direction as IN

Click Save

Modify the Request packet

Go to Administration → Network Resources → RADIUS Server Sequences.

Click on which-ever server sequence relates to the Jisc NRPS.

Click on Advanced Attribute Settings

Enable Modify Attribute in the request

Choose Add - Radius:Operator-Name - 1realm (where realm is your primary realm e.g. 1holby.local)

Click Save