RADSECProxy VLAN Assignment

### Used to add RADIUS attributes to drop all users onto VLAN 7
### The leading "'" is important as the number should be sent as a string
rewrite AddVLANAssignment {
# Tunnel-Private-Group-Id = 7
RemoveAttribute 81
AddAttribute 81:'7
# Tunnel-Type = VLAN
RemoveAttribute 64
AddAttribute 64:13
# Tunnel-Medium-Type = IEEE-802
RemoveAttribute 65
AddAttribute 65:6
# Filter-Id = 7
RemoveAttribute 11
AddAttribute 11:'7
}
server roaming0.govroam.uk {
type = udp
secret "secret"
StatusServer minimal
RewriteIn AddVLANAssignment
}
server roaming1.govroam.uk {
type = udp
secret "secret"
StatusServer minimal
RewriteIn AddVLANAssignment
}
server roaming2.govroam.uk {
type = udp
secret "secret"
StatusServer minimal
RewriteIn AddVLANAssignment
}
server roaming3.govroam.uk {
type = udp
secret "secret"
StatusServer minimal
RewriteIn AddVLANAssignment
}